WIMAX TUTORIAL 


BM622 2010 CHANGE MAC

start > run > cmd > telnet 192.168.1.1
username:wimax
password:wimax820
setallmacaddr (mac address here)
setserialnum (18 digits serial here)
restoredef



BM622 2011 CHANGE MAC

1.PLUG YOUR MODEM IN TO THE COMPUTER W8 UNTIL CONNECTED TO YOUR PC
2.ENABLE MUNA NATIN TELNET SA ADMIN.. 
3.OPEN BM622 DECODER ,,,,LINK....http://www.mediafire.com/?4mbr1a8y0oqm7a1
4.OPEN BROWSER TYPE 192.168.1.1 (ENTER) LOGIN: ADMIN PASS: UNG NA GENERATED NG BM622 DECODER
5.PAG PASOK NA SA ADMIN... PUNTA SA ACL TAPOS CHECK UNG TELNET SA LAN THEN APPLY.. (TELNET NA TAU)
6.GO TO CMD TYPE TELNET 192.168.1.1 THEN ENTER
7.LOGIN: Firefly PASS: $P4mb1h1r4N4m4nT0!! then enter
ATP>display allmacaddr (show base mac ) 
Current WAN Mac:XX:XX:XX:XX:XX:XX
Current Lan Mac:XX:XX:XX:XX:XX:XX
ATP>xiugai allmacdizhi XX:XX:XX:XX:XX:XX (input d2 present mac na lalagay mo ) hen enter
WAN MAC ADDRESS UPDATE SUCCESS xx:xx:xx:xx:xx:xx
LAN MAC ADDRESS UPDATE SUCCESS xx:xx:xx:xx:xx:xxX
ATP>restoredef (enter)



BM622i 2010 CHANGE MAC 

Login wimax
Passwordwimax820
ATPdiag set macaddr XXXXXXXXXXXX
set Lan mac address success
Lan mac address updated XXXXXXXXXXXX
set Lan Mac address Sucess
Wan mac address updated XXXXXXXXXXXX
ATP diag restore default



BM622i 2011 CHANGE MAC


1st po download nyo to...
http://www.mediafire.com/?68zl6uyztttt8bm 
2nd: connect nyo bm622i nyo sa pc
3rd run nyo yung firmware upgrader pero wag nyo po i upgrade..yaan nyo lang nakaopen..
4th: go to>start>run>cmd tpos type nyo telnet then enter
5th: after type nang telnet type nyo o 192.168.254.1 
6th: LOGIN: Firefly PASS: $P4mb1h1r4N4m4nT0!! then enter
7th: ATP>xiugai macdizhi XX:XX:XX:XX:XX:XX (yan po yung mac na ilalagay nyo)
8th: ATP>diag restore default


